1.  QUICK  STEPS TO PROGRAM THE M2000

Connection between PC and M2000

•	Connect the PC and the M2000  using a serial RS232
        crossover cable as described in section 2  of
        PREPARING FOR PROGRAMMING , and on the facing  diagram .  

On the M2000 

•	Place the indicator in calibration mode 
        and execute command 255, followed by
        pressing button 1 and pressing Tare.
•	The M2000 is  now ready to be programmed.  
 
If  the above sequence is not possible follow the steps below

•	Unplug power from the M2000 
•	With the indicator in the off state push an hold down the CAL button on the M2000 indicator key pad
•	Apply power to the indicator
•	If you hear a short beep followed by a pause, followed by two more short beeps – the indicator is ready to accept a new program
•	If  the above steps were not successful, please contact customer support.

On the PC computer 

•	The very first step is to select the Serial port to use with this application

•	Press the CONNECT M2000 button to establish a  communications
        link between the PC and the M2000 indicator. If the link is
        established, the green box in the lower right corner will light 
        up. If communications failed  -the box should be grayed out. In case of failure, please check the cabling and make sure that the COM port to be used for this application is in fact valid. Restart the application.

•	Select the file supplied with the upgrade package, it should be of type *.s.

•	Click on the PROGRAM button to start the programming process. This may take a while.

•	Once the programming process has been completed, the 
        M2000 may be remotely powered up using the 
        M2000 REMOTE RESET button. 

2.  PREPARING FOR PROGRAMMING
  
To program the indicator, you require a RS232 serial
cable to connect the PC to the M2000 indicator. See the opposing  diagram

The communication takes place via COM1 of the M2000 indicator.